How much bandwidth a seat costs · Worked example
Total a Plus agent with VPN and a CRM app. Leave Teams off, then add it.
128 plus 64 plus 64
Say the latency cap
Reject cellular
You can show the arithmetic from the PDF.
Sources and go deeper
Technical requirements PDF. vendor. https://documentation-be.five9.com/bundle/five9-technical-requirements/raw/resource/enus/five9-technical-requirements.pdf. last checked 2026-10.
