TLS, and ports that are not universal · Learn it in 5 minutes
Unencrypted APIs are not the story. TLS 1.2 is required. TLS 1.1 is not supported. The requirements also list TLS 1.3 inbound ciphers: AES-128-GCM, AES-256-GCM, and CHACHA20.
Studio portal hosts and Studio SIP ports live in the Studio section of that PDF: UDP 5060, TCP 5061 described as beta, proxy UDP 5189 and TCP 5161, a legacy UDP 5188, plus RTP ranges. Do not paste those Studio numbers onto every VCC ITSP trunk. If the trunk guide does not say them, they are not the trunk.
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